; Not all Meade scopes support all commands,  as indicated by bit flags
; in column 19.  Bit flags are: 1 = AutoStar; 2 = LX200 < 16"; 4 = LX 16";
; 8 = GPS scopes,  ORred together.  So F=supported on all scopes;
; E = supported on all but AutoStar,  etc.
;
2710 :Aa#         8 Automatic alignment (GPS only)
2711 :AL#         F Set Land alignment
2712 :AP#         F Set Polar alignment
2713 :AA#         F Set Alt/Az alignment
2714 :B+#         F Increase reticle brightness
2715 :B-#         F Decrease reticle brightness
2716 :B0#         F Reticle flash rate = 0
2717 :B1#         F Reticle flash rate = 1
2718 :B2#         F Reticle flash rate = 2
2719 :B3#         F Reticle flash rate = 3
2720 :B4#         9 Reticle flash rate = 4 (Autostar, GPS)
2721 :B5#         9 Reticle flash rate = 5 (Autostar, GPS)
2722 :B6#         9 Reticle flash rate = 6 (Autostar, GPS)
2723 :B7#         9 Reticle flash rate = 7 (Autostar, GPS)
2724 :B8#         9 Reticle flash rate = 8 (Autostar, GPS)
2725 :B9#         9 Reticle flash rate = 9 (Autostar, GPS)
2726 :f+#         4 Turn on tube exhaust fan (LX 16")
2727 :f-#         4 Turn off tube exhaust fan (LX 16")
2728 :f+#         8 Turn on power to accessor panel (GPS)
2729 :f-#         8 Turn off power to accessor panel (GPS)
2730 :ff#       s 8 Get optical tube temp (GPS)
2731 :FF#:F+#     F Focus in fast
2732 :FS#:F+#     F Focus in slow
2733 :FQ#         F Stop focuser
2734 :FF#:F-#     F Focus out fast
2735 :FS#:F-#     F Focus out slow
2736 :F1#         9 Focus speed 1 (Autostar, GPS)
2737 :F2#         9 Focus speed 2 (Autostar, GPS)
2738 :F3#         9 Focus speed 3 (Autostar, GPS)
2739 :F4#         9 Focus speed 4 (Autostar, GPS)
2740 :g+#         8 Turn on GPS (GPS)
2741 :g-#         8 Turn off GPS (GPS)
2742 :gT#         8 Initialize from GPS (GPS)
2743 :hS#         C Seek home & store posn (GPS & 16")
2744 :hF#         C Seek home & realign (GPS & 16")
2745 :hN#         8 Sleep telescope (GPS)
2746 :hW#         8 Wake up telescope (GPS)
2747 :hP#         D Slew to Park position (Autostar, GPS, 16")
2748 :I#          8 Restart scope (GPS)
2749 :Me#         F Slew to East
2750 :Mw#         F Slew to West
2751 :Mn#         F Slew to North
2752 :Ms#         F Slew to South
2753 :Q#          F Halt slewing
2754 :P#        s F Toggle to High-Precision Pointing mode
2755 :r+#         C Turn on Field Derotator (GPS, 16")
2756 :r-#         C Turn off Field Derotator (GPS, 16")
2757 :RS#         F Slew (fastest) rate
2758 :RM#         F Find (2nd fastest) slew rate
2759 :RC#         F Centering (2nd slowest) slew rate
2760 :RG#         F Guiding (slowest) slew rate
2761 :$Q#         E Toggle Smart Drive PEC on both axes (all but AutoStar)
2762 :$QA+#       8 Turn Dec/Alt PEC on (GPS)
2763 :$QA-#       8 Turn Dec/Alt PEC off (GPS)
2764 :$QZ+#       8 Turn RA/Azim PEC on (GPS)
2765 :$QZ-#       8 Turn RA/Azim PEC off (GPS)
2766 :GZ#       s F Get azimuth
2767 :GS#       s F Get sidereal time
2768 :GT#       s F Get tracking rate
2769 :U#          F Toggle high-precision coordinates mode
